TALK 2 STUDIO
PLEASE NOTE CHANGES / CORRECTIONS ON THIS SHEET

Block Number--Talk2-A1
Destination Block--Term wall-A9
Location--TALK 2 ROOM INPUTS

Clip	Left	Right
Number	Function	Function                                    

01-03	REMOTE 1 LEFT	REMOTE 1 RIGHT
04-06	REMOTE 2 LEFT	REMOTE 2 RIGHT
07-09	WWDJ Aserv mix Left to rem 3	WWDJ Aserv mix Right to rem 3
10-12	WMCA Aserv mix Left to rem 4	WMCA Aserv mix Right to rem 4
13-15	Prod 2 Stu Mon out L to rem 5in	Prod 2 Stu Mon out R to rem 5in
16-18	
19-21	DJ PGM MULT LEFT	DJ PGM MULT RIGHT
22-24	MCA PGM MULT LEFT	MCA PGM MULT RIGHT
25-27	
28-30	HYBRID 1 OUT	HYBRID 2 OUT
31-33
34-36
37-39
40-42
-----	Talk 2 block spare clips
43-45	CHANNEL 5 A IN LEFT <<Hybrid 1>>	CHANNEL 5 B IN LEFT
46-48	CHANNEL 5 A IN RIGHT<<Hybrid 1>>	CHANNEL 5 B IN RIGHT
49,50

-----	Master control block spare clips
43-45	Talk 2pgm Mult L	Talk 2pgm Mult R (frm b9 block)
46-48	Talk 2pgm Mult L	Talk 2pgm Mult R (frm b9 block)
49,50

Block Number--Talk2-A2
Destination Block--Term wall-B9
Location--TALK 2 ROOM OUTPUTS

Clip	Left	Right
Number	Function	Function                                    

01-03	TALK 2 LEFT PROGRAM	TALK 2 RIGHT PROGRAM
04-06	TALK 2 LEFT AUDITION	TALK 2 RIGHT AUDITION
07-09	TALK 2 LEFT UTILITY	TALK 2 RIGHT UTILITY
10-12	TALK 2 PROGRAM MIX -(UB)(telos)	TALK 2 MONO PGM (TELOS MOH)
13-15	MIC 1 DA 1-1	MIC 2 DA 2-1
16-18	MIC 3 DA 3-1	MIC 4 DA 4-1
119-21	MIC 1 DA 1-2	MIC 2 DA 2-2
22-24	MIC 3 DA 3-2	MIC 4 DA 4-2
25-27	Aud Mono Mix frm Rtbk rly
28-30
31-33	Tlkbck audio T2 -> Hall (UB)
34-36	Tlkbck audio Hall -> T2
37-39	Tlkbck audio DJ -> T2	Tlkbck audio MCA -> Tlk2
40-42	Tlkbck audio T2 -> DJ	Tlkbck audio Tlk2 -> MCA
-----	Talk 2 block spare clips
43-45	CHANNEL 6 A IN LEFT <<Hybrid 2>>	CHANNEL 6 B IN LEFT
46-48	CHANNEL 6 A IN RIGHT<<Hybrid 2>>	CHANNEL 6 B IN RIGHT 
49,50

-----	Master control block spare clips
43-45
46-48
49,50

Block Number--Talk2-A3
Destination Block--Term wall-C9
Location--TALK 2 CONTROLS

Clip	Left	Right
Number	Function	Function                                    
01	ESE Clock sync +	MCA Next Wiz Lamp + 12v from mc wall
02	ESE clock sync gnd	MCA Next Wiz Lamp gnd to illuminate
03		MCA Next Wiz Com T3#4
04		MCA Next Wiz N/0
05		WDJ next wiz Lamp +12v from MC wall
06		WDJ next wiz lamp gnd to illum
07		WDJ next wiz com T3#3
08		WDJ next wiz N/O
09
10
11			Go to break light relay 12v+	
12			Go to break light relay 12v- gnd to act.
13
14
15
16
17
18
19
20
21
22
23
24
25
26
27
28
29	Hall scnr tlkbck logic
30	Hall scnr tlkbck logic
31	tlkbck cntl FROM DJ
32	tlkbck cntl FROM MCA
33
34
35	scnr mic preamp +24vdc
36	scnr mic preamp -24vdc
37	scnr mon spkr +6vdc
38	scnr mon spkr -6vdc
39
40
41
42
43	Left warning light	Left warning light, screener
44	Left warning light	Left warning light, screener
45	Middle warning light	Middle warning light, screener
46	Middle warning light	Middle warning light, screener
47 	Right warning light 	Right warning light, screener
48	Right warning light 	Right warning light, screener
49	+24v to on air lights relay
50	-24v to on air lights relay

Block Number--Talk2-A4
Destination Block--Term wall-D9
Location--TALK 2 TELEPHONES / AUX

Clip	Left	Right
Number	Function	Function                                    

01	Telos Control 1 Blue	
02	Telos Control 1 Yellow	
03	Telos Control 1 Green	
04	Telos Control 1 Red	
05	Telos Control 1 Black	
06	Telos Control 1 White	
07	Tls Aux phn (dj/hall screener)	
08	Tls Aux phn (dj/hall screener)	
09	TLS AUX PHN (TLK STU/Hall Wall)	RS-232 T2 SCRN PC<>MCA SCRN PC-B
10	TLS AUX PHN (TLK STU/Hall Wall)	RS-232 T2 SCRN PC<>MCA SCRN PC-B
11	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-R
12	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-O
13	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-Y
14	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-G
15	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-B
16	Telrad phone	RS-232 T2 SCRN PC<>MCA SCRN PC-W
17	Telrad SLT	RS-232 DJ SCRN PC<>Hall SCRN PC
18	Telrad SLT	RS-232 DJ SCRN PC<>Hall SCRN PC
19		RS-232 DJ SCRN PC<>Hall SCRN PC
20		RS-232 DJ SCRN PC<>Hall SCRN PC
21		RS-232 DJ SCRN PC<>Hall SCRN PC
22		RS-232 DJ SCRN PC<>Hall SCRN PC
23		RS-232 DJ SCRN PC<>Hall SCRN PC
24		RS-232 DJ SCRN PC<>Hall SCRN PC
25
26
27
28
29
30
31
32
33
34
35
36
37
38
39
40
41
42
43
44
45	RS232 TELOS <> PC RED rx/tx
46	RS232 TELOS <> PC GREEN tx/rx
47	RS232 TELOS <> PC BLACK sig gnd
48	RS232 TELOS <> PC WHITE unused
49
50

Block Number--Talk2-A5
Destination Block--
Location--TALK 2 Mics da’s 

Clip	Left	Right
Number	Function	Function                                    

01	Mic 1 DA 1 +
02	Mic 1 DA 1 -
03	SHIELD
04	Mic 1 DA 2 +
05	Mic 1 DA 2 -
06	SHIELD
07	Mic 1 DA 3 + (tlkbck)>>>>>>>>>>>>	Remote Tlkbck Rly
08	Mic 1 DA 3 ->>>>>>>>>>>>>>>>>>>>>	Remote Tlkbck Rly
09	SHIELD
10	Mic 1 DA 4 +
11	Mic 1 DA 4 -
12	SHIELD
13	Mic 2 DA 1 +
14	Mic 2 DA 1 -
15	SHIELD
16	Mic 2 DA 2 +
17	Mic 2 DA 2 -
18	SHIELD
19	Mic 2 DA 3 +
20	Mic 2 DA 3 -
21	SHIELD
22	Mic 2 DA 4 +
23	Mic 2 DA 4 -
24	SHIELD
25	Mic 3 DA 1 +
26	Mic 3 DA 1 -
27	SHIELD
28	Mic 3 DA 2 +
29	Mic 3 DA 2 -
30	SHIELD
31	Mic 3 DA 3 +
32	Mic 3 DA 3 -
33	SHIELD
34	Mic 3 DA 4 +
35	Mic 3 DA 4 -
36	SHIELD
37	Mic 4 DA 1 +
38	Mic 4 DA 1 -
39	SHIELD
40	Mic 4 DA 2 +
41	Mic 4 DA 2 -
42	SHIELD
43	Mic 4 DA 3 +
44	Mic 4 DA 3 -
45	SHIELD
46	Mic 4 DA 4 +
47 	Mic 4 DA 4 -
48	SHIELD
49
50
Block Number--Talk2-B1
Destination Block--
Location--T2 audio

Clip	Left	Right
Number	Function	Function                                    

01	MIC 1A IN +	MIC 1B IN +
02	MIC 1A IN -	MIC 1B IN -
03	SHIELD	SHIELD
04	MIC 2A IN +	MIC 2B IN +
05	MIC 2A IN -	MIC 2B IN -
06	SHIELD	SHIELD
07	MIC 3A IN +	MIC 3B IN +
08	MIC 3A IN -	MIC 3B IN -
09	SHIELD	SHIELD
10	MIC 4A IN +	MIC 4B IN +
11	MIC 4A IN -	MIC 4B IN -
12	SHIELD	SHIELD
13	Mic1 +>>>>>>>>>>>>	Symetrix 528 IN+ See notes page
14	Mic1 - >>>>>>>>>>>	Symetrix 528 IN-
15	shield >>>>>>>>>>>>	Shield
16	Jump to Mic 1 IN >>>>>>>>>	Symetrix 528 OUT+
17	Jump to Mic 1 IN >>>>>>>>>	Symetrix 528 OUT-
18	Shield >>>>>>>>>>	Shield
19	
20	
21	REM SEL 1A IN Right +>>>>>>>>>>	REM SEL 1B IN Right +
22	REM SEL 1A IN Right ->>>>>>>>>>	REM SEL 1B IN Right -
23	SHIELD	SHIELD
24	REM SEL 1A IN Left +>>>>>>>>>>	REM SEL 1B IN Left +
25	REM SEL 1A IN Left ->>>>>>>>>>	REM SEL 1B IN Left -
26	SHIELD	SHIELD
27	REM SEL 2A IN Right +>>>>>>>>>>	REM SEL 2B IN Right +
28	REM SEL 2A IN Right ->>>>>>>>>>	REM SEL 2B IN Right -
29	SHIELD	SHIELD
30	REM SEL 2A IN Left +>>>>>>>>>>	REM SEL 2B IN Left +
31	REM SEL 2A IN Left ->>>>>>>>>>	REM SEL 2B IN Left -
32	SHIELD	SHIELD
33	REM SEL 3A IN Right +>>>>>>>>>>	REM SEL 3B IN Right +
34	REM SEL 3A IN Right ->>>>>>>>>>	REM SEL 3B IN Right -
35	SHIELD	SHIELD
36	REM SEL 3A IN Left +>>>>>>>>>>	REM SEL 3B IN Left +
37	REM SEL 3A IN Left ->>>>>>>>>>	REM SEL 3B IN Left -
38	SHIELD	SHIELD
39	REM SEL 4A IN Right +>>>>>>>>>>	REM SEL 4B IN Right +
40	REM SEL 4A IN Right ->>>>>>>>>>	REM SEL 4B IN Right -
41	SHIELD	SHIELD
42	REM SEL 4A IN Left +>>>>>>>>>>	REM SEL 4B IN Left +
43	REM SEL 4A IN Left ->>>>>>>>>>	REM SEL 4B IN Left -
44	SHIELD	SHIELD
45	REM SEL 5A IN Right +>>>>>>>>>>	REM SEL 5B IN Right +
46	REM SEL 5A IN Right ->>>>>>>>>>	REM SEL 5B IN Right -
47	SHIELD	SHIELD
48	REM SEL 5A IN Left +>>>>>>>>>>	REM SEL 5B IN Left +
49 	REM SEL 5A IN Left ->>>>>>>>>>	REM SEL 5B IN Left -
50	SHIELD	SHIELD

Block Number--Talk2-B2
Destination Block--
Location--

Clip	Left	Right
Number	Function	Function                                    

01	7A LEFT (+)	7A RIGHT (+)
02	7A LEFT (-)	7A RIGHT (-)
03	SHIELD	SHIELD
04	7B LEFT (+)	7B RIGHT (+)
05	7B LEFT (-)	7B RIGHT (-)
06	SHIELD	SHIELD
07	8A LEFT (+)	8A RIGHT (+)
08	8A LEFT (-)	8A RIGHT (-)
09	SHIELD	SHIELD
10	8B LEFT (+)	8B RIGHT (+)
11	8B LEFT (-)	8B RIGHT (-)
12	SHIELD	SHIELD
13	9A LEFT (+)	9A LEFT (+)
14	9A LEFT (-)	9A LEFT (-
15	SHIELD	SHIELD
16	9B LEFT +	9B RIGHT +
17	9B LEFT -	9B RIGHT -
18	SHIELD	SHIELD
19	10A LEFT +	10A RIGHT +
20	10A LEFT -	10A RIGHT -
21	SHIELD	SHIELD
22	10B LEFT +	10B RIGHT +
23	10B LEFT -	10B RIGHT -
24	SHIELD	SHIELD
25	11A LEFT +	11A RIGHT +
26	11A LEFT -	11A RIGHT -
27	SHIELD	SHIELD
28	11B LEFT +	11B RIGHT +
29	11B LEFT -	11B RIGHT -
30	SHIELD	SHIELD
31	12A LEFT +	12A RIGHT +
32	12A LEFT -	12A RIGHT -
33	SHIELD	SHIELD
34	12B LEFT +	12B RIGHT +
35	12B LEFT -	12B RIGHT -
36	SHIELD	SHIELD
37	13A LEFT +	13A RIGHT +
38	13A LEFT -	13A RIGHT -
39	SHIELD	SHIELD
40	13B LEFT +	13B RIGHT +
41	13B LEFT -	13B RIGHT -
42	SHIELD	SHIELD
43	14A LEFT +	14A RIGHT +
44	14A LEFT -	14A RIGHT -
45	SHIELD	SHIELD
46	14B LEFT +	14B RIGHT +
47	14B LEFT -	14B RIGHT -
48	SHIELD	SHIELD
49
50

Block Number--Talk2-B3
Destination Block--
Location--TALK 2

Clip	Left	Right
Number	Function	Function                                    

01	PROGRAM OUT LEFT +	PROGRAM OUT RIGHT +
02	PROGRAM OUT LEFT -	PROGRAM OUT RIGHT -
03	SHIELD	SHIELD
04	AUDITION OUT LEFT +	AUDITION OUT RIGHT +
05	AUDITION OUT LEFT -	AUDITION OUT RIGHT -
06	SHIELD	SHIELD
07	UTILITY OUT LEFT +	UTILITY OUT RIGHT +
08	UTILITY OUT LEFT -	UTILITY OUT RIGHT -
09	SHIELD	SHIELD
10	PROGRAM MONO SUM OUT +	MONO CUE OUT (UB)
11	PROGRAM MONO SUM OUT -	AUDIO GND
12	SHIELD	SHIELD
13	Aud MONO Sum out + to Rtbk rly
14	Aud MONO Sum out -
15	SHIELD
16	PROGRAM MIX- OUT (UB)	AUDITION MIX - OUT (UB)
17	AUDIO GND	AUDIO GND
18	MONITOR OUT LEFT (UB)	MONITOR OUT RIGHT (UB)
19	AUDIO GND	AUDIO GND
20	HEADPHONE OUT LEFT (UB)	HEADPHONE OUT RIGHT (UB)
21	AUDIO GND	AUDIO GND
22	STUDIO 1 MUTED OUT LEFT (UB)	STUDIO 1 MUTED OUT RIGHT (UB)
23	AUDIO GND	AUDIO GND
24	STUDIO 1 UNMUTED OUT LEFT (UB)	STUDIO 1 UNMUTED OUT RIGHT (UB)
25	AUDIO GND	AUDIO GND
26	STUDIO 2 UNMUTED OUT LEFT (UB)	STUDIO 2 UNMUTED OUT RIGHT (UB)
27	AUDIO GND	AUDIO GND
28	EXTERNAL MON IN 1 LEFT +	EXTERNAL MON IN 1 RIGHT +
29	EXTERNAL MON IN 1 LEFT -	EXTERNAL MON IN 1 RIGHT -
30	SHIELD	SHIELD
31	EXTERNAL MON IN 2 LEFT +	EXTERNAL MON IN 2 RIGHT +
32	EXTERNAL MON IN 2 LEFT -	EXTERNAL MON IN 2 RIGHT -
33	SHIELD	SHIELD
34	EXT STU MON IN LEFT (UB)	EXT STU MON IN RIGHT (UB)
35	AUDIO GND	AUDIO GND
36	REMOTE SELECT SW A LEFT OUT +	REMOTE SELECT SW A RIGHT OUT +
37	REMOTE SELECT SW A LEFT OUT -	REMOTE SELECT SW A RIGHT OUT -
38	SHIELD	SHIELD
39 	REMOTE SELECT SW B LEFT OUT +	REMOTE SELECT SW B RIGHT OUT +
40 	REMOTE SELECT SW B LEFT OUT -	REMOTE SELECT SW B RIGHT OUT - 
41	SHIELD	SHIELD
42	INTERCOM AUD FRM STUDIO 1 (UB)	INTERCOM AUD FRM STUDIO 2 (UB)
43	AUDIO GND	AUDIO GND
44
45	CR MUTE RELAY DRIVER OUT (OC)
46	LOGIC GROUND
47	STUDIO 1 MUTE RELAY DRIVER OUT (OC)
48	LOGIC GROUND
49	STUDIO 2 MUTE RELAY DRIVER OUT (OC)
50	LOGIC GROUND

Block Number--Talk2-B4
Destination Block--
Location--

Clip	Left	Right
Number	Function	Function                                    

01	MIC 1A REM CHAN ON	MIC 1B REM CHAN ON
02	MIC 1A REM CHAN OFF	MIC 1B REM CHAN OFF
03	MIC 1A CUE / TALKBACK	MIC 1B CUE / TALKBACK
04	MIC 1A COUGH MUTE	MIC 1B COUGH MUTE
05	MIC 1A LOGIC GROUND	MIC 1B LOGIC GROUND
06	MIC 2A REM CHAN ON	MIC 2B REM CHAN ON
07	MIC 2A REM CHAN OFF	MIC 2B REM CHAN OFF
08	MIC 2A CUE / TALKBACK	MIC 2B CUE / TALKBACK
09	MIC 2A COUGH MUTE	MIC 2B COUGH MUTE
10	MIC 2A LOGIC GROUND	MIC 2B LOGIC GROUND
11	MIC 3A REM CHAN ON	MIC 3B REM CHAN ON
12	MIC 3A REM CHAN OFF	MIC 3B REM CHAN OFF
13	MIC 3A CUE / TALKBACK	MIC 3B CUE / TALKBACK
14	MIC 3A COUGH MUTE	MIC 3B COUGH MUTE
15	MIC 3A LOGIC GROUND	MIC 3B LOGIC GROUND
16	MIC 4A REM CHAN ON	MIC 4B REM CHAN ON
17	MIC 4A REM CHAN OFF	MIC 4B REM CHAN OFF
18	MIC 4A CUE / TALKBACK	MIC 4B CUE / TALKBACK
19	MIC 4A COUGH MUTE	MIC 4B COUGH MUTE
20	MIC 4A LOGIC GROUND	MIC 4B LOGIC GROUND
21
22	----note; input 5 remote starts on loose 8451---
23	INPUT 6B  REMOTE START	INPUT 6A REMOTE START
24	INPUT 6B REMOTE STOP	INPUT 6A REMOTE STOP
25	INPUT 6B START / STOP COMMON	INPUT 6A START / STOP COMMON
26	INPUT 7B  REMOTE START	INPUT 7A REMOTE START
27	INPUT 7B REMOTE STOP	INPUT 7A REMOTE STOP
28	INPUT 7B START / STOP COMMON	INPUT 7A START / STOP COMMON
29	INPUT 8B REMOTE START	INPUT 8A REMOTE START
30	INPUT 8B REMOTE STOP	INPUT 8A REMOTE STOP
31	INPUT 8B START / STOP COMMON	INPUT 8A START / STOP COMMON 
32	INPUT 9B REMOTE START	INPUT 9A REMOTE START
33	INPUT 9B REMOTE STOP	INPUT 9A REMOTE STOP
34	INPUT 9B START / STOP COMMON	INPUT 9A START / STOP COMMON
35	INPUT 10B REMOTE START	INPUT 10A REMOTE START
36	INPUT 10B REMOTE STOP	INPUT 10A REMOTE STOP
37	INPUT 10B START / STOP COMMON	INPUT 10A START / STOP COMMON
38	INPUT 11B REMOTE START	INPUT 11A REMOTE START
39	INPUT 11B REMOTE STOP	INPUT 11A REMOTE STOP
40	INPUT 11B START / STOP COMMON	INPUT 11A START / STOP COMMON
41	INPUT 12B REMOTE START	INPUT 12A REMOTE START
42	INPUT 12B REMOTE STOP	INPUT 12A REMOTE STOP
43	INPUT 12B START / STOP COMMON	INPUT 12A START / STOP COMMON
44	INPUT 13B REMOTE START	INPUT 13A REMOTE START
45	INPUT 13B REMOTE STOP	INPUT 13A REMOTE STOP
46	INPUT 13B START / STOP COMMON	INPUT 13A START / STOP COMMON
47	INPUT 14B REMOTE START	INPUT 14A REMOTE START
48	INPUT 14B REMOTE STOP	INPUT 14A REMOTE STOP
49	INPUT 14B START / STOP COMMON	INPUT 14A START / STOP COMMON
50

Block Number--Talk2-B5
Destination Block--
Location--Talk 2 PR/E switch & TAPE CONTROLS

Clip	Left	Right
Number	Function	Function                                    

01-03	Input 1 Left	Input 1 Right
04-06	Input 2 Left	Input 2 Right
07-09	Input 3 Left	Input 3 Right
10-12	Input 4 Left	Input 4 Right
13-15	Input 5 Left	Input 5 Right
16-18	Output 4 Left	Output 4 Right
19	TAPE 1	REC NO CONTACTS	TAPE 3
20	TAPE 1	REC NO CONTACTS	TAPE 3
21	TAPE 1	FWD NO CONTACTS	TAPE 3
22	TAPE 1	FWD NO CONTACTS	TAPE 3
23	TAPE 1	RWD NO CONTACTS	TAPE 3
24	TAPE 1	RWD NO CONTACTS	TAPE 3
25	TAPE 1	PLAY NO CONTACTS	TAPE 3 MCA Wiz next
26	TAPE 1	PLAY NO CONTACTS	TAPE 3 MCA wiz next
27	TAPE 1	STOP NO CONTACTS	TAPE 3 WDJ wiz next
28	TAPE 1	STOP NO CONTACTS	TAPE 3 WDJ wiz next
29	TAPE 1 REC LIGHT +	TAPE 3 REC LIGHT - gnd to illuminate
30	TAPE 1 FWD LIGHT +	TAPE 3 FWD LIGHT -
31	TAPE 1 REW LIGHT +	TAPE 3 REW LIGHT -
32	TAPE 1 PLAY LIGHT +	TAPE 3 PLAY LIGHT - mca wiz next
33	TAPE 1 STOP LIGHT +	TAPE 3 STOP LIGHT - WDJ wiz next
34	TAPE 1 LIGHTS COM -	TAPE 3 LIGHTS COM +12VDC on mc wall
35	TAPE 2	REC NO CONTACTS	TAPE 4-blue
36	TAPE 2	REC NO CONTACTS	TAPE 4
37	TAPE 2	FWD NO CONTACTS	TAPE 4-red
38	TAPE 2	FWD NO CONTACTS	TAPE 4
39	TAPE 2	RWD NO CONTACTS	TAPE 4-orange
40	TAPE 2	RWD NO CONTACTS	TAPE 4
41	TAPE 2	PLAY NO CONTACTS	TAPE 4-brown
42	TAPE 2	PLAY NO CONTACTS	TAPE 4
43	TAPE 2	STOP NO CONTACTS	TAPE 4-yellow
44	TAPE 2	STOP NO CONTACTS	TAPE 4
45	TAPE 2	REC LIGHT +	TAPE 4
46	TAPE 2	FWD LIGHT +	TAPE 4
47	TAPE 2	REW LIGHT +	TAPE 4
48	TAPE 2	PLAY LIGHT +	TAPE 4
49	TAPE 2	STOP LIGHT +	TAPE 4
50	TAPE 2	LIGHTS COM -	TAPE 4

Block Number--Talk2 C1
Destination Block--
Location--TALK 2 Audio Pairs TO DJ SCREEN POSITION

Clip	Left	Right
Number	Function	Function                                    

01-03
04-06
07-09
10-12
13-15
16-18	
19-21
22-24
25-27		
28-30
31-33
34-36
37-39
40-42	Stu 1 Unmuted mon out to scrnr	tlkbck audio frm scrnr
43
44
45
46	Call Logic to studio 2	TBK to MCA relay coil xistor
47	Call Logic to studio 1	TBK to DJ relay coil xistor
48	Call Logic From Studio 2	TBK frm MCA relay coil
49	Call Logic Frm Stu 1/dj scrn	TBK frm DJ rly coil/hall scrn
50	Audio gnd	Audio Gnd

Block Number--Talk2 C2
Destination Block--BETWEEN DJ SCREEN & TALK 2 POSITIONS
Location--DJ SCREENER POSITION

Clip	Left	Right
Number	Function	Function                                    
01	TELOS SCREENER PHN	Tlkbck Logic
02	TELOS SCREENER PHN	Tlkbck Logic
03
04
05
06
07
08
09	RS-232 T2 SCRN PC<>MCA SCRN PC-B	
10	RS-232 T2 SCRN PC<>MCA SCRN PC-B
11	RS-232 T2 SCRN PC<>MCA SCRN PC-R
12	RS-232 T2 SCRN PC<>MCA SCRN PC-O
13	RS-232 T2 SCRN PC<>MCA SCRN PC-Y
14	RS-232 T2 SCRN PC<>MCA SCRN PC-G
15	RS-232 T2 SCRN PC<>MCA SCRN PC-B
16	RS-232 T2 SCRN PC<>MCA SCRN PC-W
17
18
19
20	RS-232 DJ SCRN PC<>HALL SCRN PC
21	RS-232 DJ SCRN PC<>HALL SCRN PC
22	RS-232 DJ SCRN PC<>HALL SCRN PC
23	RS-232 DJ SCRN PC<>HALL SCRN PC
24	RS-232 DJ SCRN PC<>HALL SCRN PC
25	RS-232 DJ SCRN PC<>HALL SCRN PC
26	RS-232 DJ SCRN PC<>HALL SCRN PC
27	RS-232 DJ SCRN PC<>HALL SCRN PC
28
29
30
31	Scrn Mic Preamp +24vdc	Scrn Mic Preamp +24vdc
32	Scrn Mic preamp -24vdc	Scrn Mic preamp -24vdc
33	Scrn Mon spkr +6vdc	Scrn Mon spkr +6vdc
34	Scrn Mon spkr -6vdc	Scrn Mon spkr -6vdc	
35
36
37
38
39
40
41
42
43		Left warning light
44		Left warning light
45	RS232 TELOS <> PC RED rx/tx	Middle warning light
46	RS232 TELOS <> PC GREEN tx/rx	Middle warning light
47	RS232 TELOS <> PC BLACK sig gnd 	Right warning light
48	RS232 TELOS <> PC WHITE unused 	Right warning light
49	
50

Block Number--Term Wall E-9
Destination Block--Hall screener Wk Station
Location--Master control / Hall desk

Clip	Left	Right
Number	Function	Function                                    

01		RS-232 DJ SCRN PC<>HALL SCRN PC 
02		RS-232 DJ SCRN PC<>HALL SCRN PC 
03		RS-232 DJ SCRN PC<>HALL SCRN PC
04		RS-232 DJ SCRN PC<>HALL SCRN PC
05		RS-232 DJ SCRN PC<>HALL SCRN PC
06		RS-232 DJ SCRN PC<>HALL SCRN PC
07		RS-232 DJ SCRN PC<>HALL SCRN PC
08		RS-232 DJ SCRN PC<>HALL SCRN PC
09
10
11		Mic Preamp +24vdc
12		Mic preamp -24vdc
13		Hall Scnr -> T2 audio +
14		Hall Scnr -> T2 audio gnd
15		Hall tlkbck logic contact
16		Hall tlkbck logic contact
17		Hall mon spkr +6vdc
18		Hall mon spkr -6vdc
19		Hall mon audio +
20		Hall mon audio -
21		Intercom/ radioshack
22		Intercom/ radioshack
23
24
25
26
27
28
29
30
31
32
33
34
35
36
37
38
39
40
41
42
43
44
45
46
47
48
49		Tlos scrn phn hall/dj Paralleled	
50		Tlos Scrn phn hall/dj Paralleled